FedBizOpps

**Combined Synopsis/Solicitation Notice**

**\***

**\***

**\***

**\***

**\***

**\***

**\***

**CLASSIFICATION CODE**

**SUBJECT**

**CONTRACTING OFFICE'S**

**ZIP-CODE**

**SOLICITATION NUMBER**

**RESPONSE DATE (MM-DD-YYYY)**

**ARCHIVE**

**DAYS AFTER THE RESPONSE DATE**

**RECOVERY ACT FUNDS**

**SET-ASIDE**

**NAICS CODE**

**CONTRACTING OFFICE**

**ADDRESS**

**POINT OF CONTACT**

(POC Information Automatically Filled from

User Profile Unless Entered)

**DESCRIPTION**

**\***

**See Attachment**

**AGENCY'S URL**

**URL DESCRIPTION**

**AGENCY CONTACT'S EMAIL**

**ADDRESS**

**EMAIL DESCRIPTION**

**ADDRESS**

**POSTAL CODE**

**COUNTRY**

**ADDITIONAL INFORMATION**

**GENERAL INFORMATION**

**PLACE OF PERFORMANCE**

**\* = Required Field**

FedBizOpps Combined Synopsis/Solicitation Notice

Rev. March 2010

62

583-17-2-663-0407- Lights for Main Campus and CSR

48105

VA250-17-Q-1224

09-21-2017

30

N

335110

Department of Veterans Affairs

Ann Arbor Healthcare System

Network Contracting Office 10

2215 Fuller Road

Ann Arbor MI 48105

Kellie Konopinski

Kellie.Konopinski@va.gov

VA Medical Center

1481 W. 10th Street

Indianapolis, IN

46202

This is a combined synopsis/solicitation for commercial items prepared in accordance with the format in FAR Subpart 12.6, as supplemented with additional information included in this notice. This announcement constitutes the only solicitation; quotes are being requested and a written solicitation will not be issued.

This solicitation RFQ-VA250-17-Q-1224 is issued as a request for quote (RFQ). This solicitation document and incorporated provisions and clauses are those in effect through Federal Acquisition Circular (FAC) 2005-94, 2005-95/ 01-19-2017. The North American Industry Classification System (NAICS) number is 335110 and the business size standard is 1250 employees.

STATEMENT OF NEED

|  |  |  |  |
| --- | --- | --- | --- |
| **ITEM NUMBER** | **DESCRIPTION OF SUPPLIES/SERVICES** | **QUANTITY** | **UNIT** |
| **0001** | LSI SFCM WB LED PL1 40 BRZ (LED LIGHTS) | 15.00 | EA |
| **0002** | LSI SFCM WB LED PL1 40 UE BRZ (LED LIGHTS) | 10.00 | EA |
| **0003** | 6 MULTI-CHIP 13W LL LED TRUNNION MTG (LED LIGHTS) | 3.00 | EA |
| **0004** | CEILING MOUNT VRC LED RETROFIT (LED LIGHTS) | 5.00 | EA |
| **0005** | LITHONIA OLF LED P1 50K MVOLT THK (LED LIGHTS) | 1.00 | EA |

General:

Contractor to provide 10 LED Traditional Wallpacks (Large Cut-Off). 15 LED Traditional Wallpacks (Medium Cut-off), 5 VRC LED LED lights(Canopy), 3 LED Floodlights and 1LED Flood Luminaire associated equipment for the Veterans Affairs, Richard L. Roudebush VA Medical Center, 1481 W 10th Street, Indianapolis, IN 46202.

Delivery Hours:

Normal delivery would be between the hours of 8:00 am ET and 4:30 pm ET.

Required products by contractor:

1. Provide each of the following materials:

* 15 LED Traditional Wall Packs Medium Cut-Off (SFCM)
* 10 LED Traditional Wall Packs Large Cur-Off (SFCL)
* 3 FXLED78TN/PCT Flood Lights
* 1 OFL Size 1 LED Flood Luminaire
* 5 VRC LED Canopy/Ceiling Luminaire

Light Specifications:

**OFL Size 1 LED Flood Luminaire**

Lithonia

EPA 0.6 ft.

Depth: 8.3”

Width: 7”

Height 6.9”

Weight 5 lbs.

* Housing is completely sealed for moisture
* Suitable for replacing 150W Metal Halide
* UL Certified to US Standards
* Mvolt driver operates on any line voltage from 120-277V (50-60 Hz)
* 4000 Lumens
* 50,000 hours of expected service life
* Luminaire is IP65 rated
* Rated for -40C

Accessories:

* OFL1WG Wire Guard Accessory
* OFL1VG Vandal Guard Accessory
* DSXF1/2TS Slipfitter attachment

**FXLED78TN/PCT Flood Lights**

Rab Lighting

Watts: 78W

Color temp: 4000K

Color Accuracy: 81 CRI

L70 Lifespan: 100000

Lumens: 6734

Efficacy: 86 LPW

* 100,000 hour lifespan based on IES LM-80 results and TM-21 calculations
* LED lights are 6 multi-chip, 13 watt high output, long-life LED’s
* 3-step MacAdam Ellipse binning to achieve consistent fixture to fixture color
* LED color temperature is warrantied to shift no more than 200K in CCT over 5 years
* RAB’s range of CCT follows guidelines of ANSI c78.377-2015
* IP Rating of IP66 for dust and water
* Suitable for use in 40C ambient temperatures
* Minimum starting temperature is -40C
* Die-cast aluminum housing and door frame
* Heavy-duty trunnion-metallized polycarbonate
* High-temperature silicone gaskets

Electrical

* Constant current, class 2, 2000mA, 100-277V, 50-60Hz, 1.1A, Power Factor 99%
* THD 4.3% at 120v, 13.9% at 277v
* 4kV surge protection
* 120-277 twistlock photocell included

**VRC LED Canopy/Ceiling Luminaire outside lights**

Width: 12-3/8

Height: 8-3/4

Depth: 12-3/8

Weight: 7.5 lbs

* 41 watt LED ceiling light delivers 3389 lumens
* Energy replacement for 250w MH canopy/ceiling lights
* VRC LED provides years of maintenance-free general illumination
* Two high-powered LED’s provides 3400 lumens, includes a MVOLT (120-277V)
* High-performance LED’s maintain 84% or life for 100,000 hours of service life
* UL Listed for U.S. safety standards for wet locations

**LSI LED Traditional Wallpacks Lights (large Cut-off)**

Dimensions: 13.7” x 18.5” x 9.1”

Weight: 9.48 lbs

CRI 85

Lumens per Watt: 105

Lumens 10,426

System Wattage 99W

Color Temperature 4000k

* Precision die-cast aluminum housing
* Class 2 driver has universal voltage (120-277v, 50/60 Hz) input. 10Kv surge protection standard
* Dimming: 0-10 volt dimming, standard
* Operating temperature -35 through 40C
* Photocell 120-277 photocell with cover
* Luminaire features a back plate designed to be easily mounted to a 4” square electrical box

**LED Traditional Wallpacks Medium Cut-off (SFCM)**

Color Temperature: 4000k

System Wattage 33W

Replaces 175/150w HID

Lumens 3533 lms

Lumens per Watt 107 ipw

CRI 85

Dimensions 11.4” x 14.2” x9.1”

Precision die-cast aluminum housing with stainless steel hardware

Select high-performance LEDs

Reference below Technical/lumen Output chart

Class 2 driver has universal voltage (120-277v, 50/60 Hz) input. 10 Kv surge protection standard

0-10 volt dimming, standard

-35 through 40C

120-277 photocell standard with cover

Highly specular forward throw relector

Chip and fade resistant powder coat finish

50,000 hours

UL listed to the US for wet locations

* Delivery is to:

|  |
| --- |
| VA Medical Center  1481 West 10th Street  Indianapolis, IN 46202 |

The proposed contract listed here is Set-aside 100% for Small Business. FOB destination.

Offerors must comply with all instructions contained in provision 52.212-1, Instructions to Offerors-Commercial, applies to this acquisition. 52.203-98, 52.204-22

52.212-2, Evaluation - Commercial Items: FAR provision 52.212-2 does not apply to this solicitation. Award will be based on lowest price technically acceptable offer.

52.212-3, Offeror Representations and Certifications-Commercial Items, a completed copy of this provision shall be submitted with the offer unless SAM registered which must be noted in the quotation.

52.212-4, Contract Terms and Conditions-Commercial Items. The following additional clauses apply: 52,203-99, 52.232-40, 852.203-70, 852.232-72

52.212-5, Contract Terms and Conditions Required to Implement Statutes or Executive Orders-Commercial Items, to include clauses: 52.219-6, 52.219-28, 52.222-3, 52.222-19, 52.222-21; 52.222-50, 52.223-18, 52.225-1; 52.225-13, 52.232-34

RESPONSES ARE DUE Thursday, September 21, 2017, by 4:30 p.m. eastern standard time (est). Electronic offers will be accepted – Kellie Konopinski, e-mail [Kellie.Konopinski@va.gov](mailto:Kellie.Konopinski@va.gov).

Point of contact for this solicitation is Kellie Konopinski, 734-222-4330 or e-mail [Kellie.Konopinski@va.gov](mailto:Kellie.Konopinski@va.gov). All Inquires must be in writing.